NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** EGYPT  **If applicable, name of local government involved (Article 3.2 and 7.2):** |
| **2.** | **Agency responsible:**  Egyptian Organization for Standardization and Quality  16 Tadreeb El-Modarrebeen St., Ameriya, Cairo – Egypt  E-mail: [eos@idsc.net.eg](mailto:eos@idsc.net.eg) / [eos.tbt@eos.org.eg](mailto:eos.tbt@eos.org.eg)  Website: <http://www.eos.org.eg>  Tel.: + (202) 22845528  Fax: + (202) 22845504  **Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:** |
| **3.** | **Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Lifejackets, buoyancy aids and flotation devices (ICS code(s): 13.340.70); Outdoor and water sports equipment (ICS code(s): 97.220.40) |
| **5.** | **Title, number of pages and language(s) of the notified document:** Draft of Egyptian standard ES "buoyant aids for swimming instruction part1: safety requirements and test methods for buoyant aids to be worn"; (55 page(s), in Arabic) |
| **6.** | **Description of content:** This draft of Egyptian standard specifies safety and in water performance requirements for construction, sizing, marking and information supplied by the manufacturer for swimming aids intended to ensure a degree of buoyancy to assist beginners with movement through the water while learning to swim or while learning part of a swimming stroke. It also gives methods of test for verification of these requirements.  This document applies only to swimming devices that are designed to be worn, to be securely attached to the body and which have either inherent buoyancy or can be inflated. It only applies to class B swimming devices intended to introduce the user to the range of swimming strokes.  It does not apply to class A or class C swimming devices, to pull buoys, swim rings, lifebuoys, buoyancy aids, lifejackets or aquatic toys.  This document is not applicable for products known as 'baby neck rings' aiming to keep the user's airways above the water level.  Worth mentioning is that this draft standard is technically identical with EN 13138-1/2012+AC 2022 |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Safety and quality requirements. |
| **8.** | **Relevant documents:**  EN 13138-1/2012+AC 2022 |
| **9.** | **Proposed date of adoption:** To be determined  **Proposed date of entry into force:** To be determined |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [X] or address, telephone and fax numbers and email and website addresses, if available, of other body:**  Egyptian Organization for Standardization and Quality  Address: 16 Tadreeb El-Modarrebeen St., Ameriya, Cairo- Egypt  E-mail: [eos@idsc.net.eg](mailto:eos@idsc.net.eg) / [eos.tbt@eos.org.eg](mailto:eos.tbt@eos.org.eg)  Website: <http://www.eos.org.eg>  Tel: + (202) 22845528  Fax: + (202) 22845504 |