NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** EGYPT  **If applicable, name of local government involved (Article 3.2 and 7.2):** |
| **2.** | **Agency responsible:**  Egyptian Organization for Standardization and Quality  16 Tadreeb El-Modarrebeen St., Ameriya, Cairo – Egypt  E-mail: [eos@idsc.net.eg](mailto:eos@idsc.net.eg) / [eos.tbt@eos.org.eg](mailto:eos.tbt@eos.org.eg)  Website: <http://www.eos.org.eg>  Tel.: + (202) 22845528  Fax: + (202) 22845504  **Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:** |
| **3.** | **Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Fire-fighting (ICS code(s): 13.220.10) |
| **5.** | **Title, number of pages and language(s) of the notified document:** Draft of Egyptian standard for "Fire-fighting pumps. Fire-fighting centrifugal pumps without primer Classification, general and safety requirements";; (39 page(s), in English) |
| **6.** | **Description of content:** This draft of Egyptian standard applies to centrifugal pumps without priming devices for fire-fighting use designed as  - floating pumps (FPN F),  - submersible pumps (FPN S) or  - boosted pumps (FPN B).  Fire-fighting centrifugal pumps without primer are defined as terminated by their inlet and outlet connections as well as by their shaft ends.  This document applies for fire-fighting centrifugal pumps without priming devices for use under ambient temperatures between -15 °C and 40 °C.  NOTE 1 For special conditions, -30° C; see 6.11.  This document does not apply to fire-fighting centrifugal pumps without primer of which the only power source is directly applied manual effort.  Worth mentioning is that this Draft standard adopts the technical content of BS EN 14710-1:2005+A2:2008 |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Safety and Quality requirements |
| **8.** | **Relevant documents:**  BS EN 14710-1:2005+A2:2008 |
| **9.** | **Proposed date of adoption:** To be determined  **Proposed date of entry into force:** To be determined |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [X] or address, telephone and fax numbers and email and website addresses, if available, of other body:**  Egyptian Organization for Standardization and Quality  Address: 16 Tadreeb El-Modarrebeen St., Ameriya, Cairo- Egypt  E-mail: [eos@idsc.net.eg](mailto:eos@idsc.net.eg) / [eos.tbt@eos.org.eg](mailto:eos.tbt@eos.org.eg)  Website: <http://www.eos.org.eg>  Tel: + (202) 22845528  Fax: + (202) 22845504 |